(module PARTICLE_PHOTON_TEMPLATE_NO_STANDOFF (layer F.Cu) (tedit 5962EE59)
  (attr virtual)
  (fp_text reference >NAME (at 0 -11.43) (layer F.SilkS)
    (effects (font (size 0.8128 0.8128) (thickness 0.1524)))
  )
  (fp_text value >VALUE (at 0 13.716) (layer F.SilkS)
    (effects (font (size 0.8128 0.8128) (thickness 0.1524)))
  )
  (fp_line (start 10.16 16.51) (end 8.89 19.05) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 10.16 16.51) (end 7.62 16.51) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 7.62 16.51) (end 7.62 14.47546) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 7.62 14.47546) (end -2.0828 14.47546) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -2.0828 14.47546) (end -2.0828 19.05) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -2.0828 19.05) (end 8.89 19.05) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 3.39852 -17.4879) (end 2.99974 -17.4879) (layer Dwgs.User) (width 0.127))
  (fp_line (start -2.99974 -17.4879) (end -3.39852 -17.4879) (layer Dwgs.User) (width 0.127))
  (fp_line (start 3.39852 -17.4879) (end 3.39852 -16.7894) (layer Dwgs.User) (width 0.127))
  (fp_line (start 3.39852 -16.7894) (end 3.39852 -12.48918) (layer Dwgs.User) (width 0.127))
  (fp_line (start -3.39852 -12.48918) (end -2.19964 -12.48918) (layer Dwgs.User) (width 0.127))
  (fp_line (start -3.39852 -12.48918) (end -3.39852 -16.7894) (layer Dwgs.User) (width 0.127))
  (fp_line (start -3.39852 -16.7894) (end -3.39852 -17.4879) (layer Dwgs.User) (width 0.127))
  (fp_line (start 3.39852 -16.7894) (end -3.39852 -16.7894) (layer Dwgs.User) (width 0.127))
  (fp_line (start 2.19964 -13.88872) (end -2.19964 -13.88872) (layer Dwgs.User) (width 0.127))
  (fp_line (start -2.19964 -13.88872) (end -2.19964 -12.48918) (layer Dwgs.User) (width 0.127))
  (fp_line (start 2.19964 -13.88872) (end 2.19964 -12.48918) (layer Dwgs.User) (width 0.127))
  (fp_line (start 3.39852 -12.48918) (end 2.19964 -12.48918) (layer Dwgs.User) (width 0.127))
  (fp_line (start 3.39852 -17.4879) (end 3.99796 -18.08988) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -3.39852 -17.4879) (end -3.99796 -18.08988) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 2.99974 -17.4879) (end 2.99974 -17.88922) (layer Dwgs.User) (width 0.127))
  (fp_line (start 2.79908 -18.13814) (end -2.74828 -18.13814) (layer Dwgs.User) (width 0.127))
  (fp_line (start -2.99974 -17.93748) (end -2.99974 -17.4879) (layer Dwgs.User) (width 0.127))
  (fp_line (start -8.89 19.05) (end -10.16 16.51) (layer F.SilkS) (width 0.2032))
  (fp_line (start -10.16 16.51) (end -10.16 -16.51) (layer F.SilkS) (width 0.2032))
  (fp_line (start -10.16 -16.51) (end 10.16 -16.51) (layer F.SilkS) (width 0.2032))
  (fp_line (start 10.16 -16.51) (end 10.16 16.51) (layer F.SilkS) (width 0.2032))
  (fp_line (start 10.16 16.51) (end 8.89 19.05) (layer F.SilkS) (width 0.254))
  (fp_line (start 8.89 19.05) (end -8.89 19.05) (layer F.SilkS) (width 0.2032))
  (fp_line (start -11.43 -12.7) (end -8.89 -12.7) (layer F.Cu) (width 0.3048))
  (fp_line (start -8.89 -10.16) (end -11.43 -10.16) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 -7.62) (end -8.89 -7.62) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 -5.08) (end -8.89 -5.08) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 -2.54) (end -8.89 -2.54) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 0) (end -8.89 0) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 2.54) (end -8.89 2.54) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 5.08) (end -8.89 5.08) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 7.62) (end -8.89 7.62) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 10.16) (end -8.89 10.16) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 12.7) (end -8.89 12.7) (layer F.Cu) (width 0.3048))
  (fp_line (start -11.43 15.24) (end -8.89 15.24) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 15.24) (end 11.43 15.24) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 12.7) (end 11.43 12.7) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 10.16) (end 11.43 10.16) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 7.62) (end 11.43 7.62) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 5.08) (end 11.43 5.08) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 2.54) (end 11.43 2.54) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 0) (end 11.43 0) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 -2.54) (end 11.43 -2.54) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 -5.08) (end 11.43 -5.08) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 -7.62) (end 11.43 -7.62) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 -10.16) (end 11.43 -10.16) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 -12.7) (end 11.43 -12.7) (layer F.Cu) (width 0.3048))
  (fp_line (start 8.89 19.05) (end 10.16 16.51) (layer F.SilkS) (width 0.2032))
  (fp_line (start 10.16 16.51) (end 7.62 16.51) (layer F.SilkS) (width 0.2032))
  (fp_line (start 7.62 16.51) (end 7.62 14.47546) (layer F.SilkS) (width 0.2032))
  (fp_line (start 7.62 14.47546) (end -2.0828 14.47546) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.0828 14.47546) (end -2.0828 19.05) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.0828 19.05) (end 8.89 19.05) (layer F.SilkS) (width 0.2032))
  (fp_line (start 8.89 19.05) (end 10.16 16.51) (layer F.SilkS) (width 0.2032))
  (fp_line (start 10.16 16.51) (end 7.62 16.51) (layer F.SilkS) (width 0.2032))
  (fp_line (start 7.62 16.51) (end 7.62 14.47546) (layer F.SilkS) (width 0.2032))
  (fp_line (start 7.62 14.47546) (end -2.0828 14.47546) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.0828 14.47546) (end -2.0828 19.05) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.0828 19.05) (end 8.89 19.05) (layer F.SilkS) (width 0.2032))
  (fp_arc (start 2.76098 -17.90446) (end 2.79908 -18.13814) (angle 84.5) (layer Dwgs.User) (width 0.127))
  (fp_arc (start -2.76352 -17.90192) (end -2.99974 -17.93748) (angle 84.5) (layer Dwgs.User) (width 0.127))
  (fp_text user Keepout (at 2.54 16.51) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.0762)))
  )
  (fp_text user A0 (at -7.26186 15.0876 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user A1 (at -7.26186 12.2936 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user A2 (at -7.26186 10.0076 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user RX (at -7.26186 -5.207 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user A4 (at -7.26186 4.9276 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user A3 (at -7.26186 7.4168 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user A5 (at -7.26186 2.3876 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user DAC (at -7.23646 0.0254 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user WKP (at -7.26186 -2.8448 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user D0 (at 7.23646 15.3924 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user D1 (at 7.23646 12.9286 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user D2 (at 7.23646 10.3124 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user D3 (at 7.23646 7.7724 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user D4 (at 7.23646 5.207 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user D5 (at 7.23646 2.6924 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user D6 (at 7.23646 0.1524 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user D7 (at 7.23646 -2.3876 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user GND (at 7.21106 -4.7244 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user VBAT (at 7.21106 -7.4676 270) (layer Dwgs.User)
    (effects (font (size 0.762 0.762) (thickness 0.1016)))
  )
  (fp_text user RST (at 7.21106 -10.0838 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user 3V3 (at 7.23646 -12.5476 270) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user TX (at -7.26186 -7.7978 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user GND (at -7.26186 -10.33526 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user VIN (at -7.26186 -12.9794 90) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1016)))
  )
  (fp_text user GND (at -14.351 -10.16) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user TX (at -13.843 -7.62) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user RX (at -13.843 -5.08) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user WKP (at -14.351 -2.54) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user DAC (at -14.351 0) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user A5 (at -13.843 2.54) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user A4 (at -13.843 5.08) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user A3 (at -13.843 7.62) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user A2 (at -13.843 10.16) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user A1 (at -13.843 12.7) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user D1 (at 13.843 12.7) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user D2 (at 13.843 10.16) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user D3 (at 13.843 7.62) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user D4 (at 13.843 5.08) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user D5 (at 13.843 2.54) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user D6 (at 13.843 0) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user D7 (at 13.843 -2.54) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user GND (at 14.351 -5.08) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user VBT (at 14.351 -7.62) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user RST (at 14.351 -10.16) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 3V3 (at 14.2748 -12.6746) (layer F.SilkS)
    (effects (font (size 0.9652 0.9652) (thickness 0.1524)))
  )
  (fp_text user VIN (at -14.097 -12.7 180) (layer F.SilkS)
    (effects (font (size 0.9652 0.9652) (thickness 0.1524)))
  )
  (fp_text user A0 (at -13.843 15.24 180) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user D0 (at 13.7922 15.24) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user VIN (at -14.6812 -12.6746) (layer B.SilkS)
    (effects (font (size 0.9652 0.9652) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user GND (at -14.605 -10.16) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user TX (at -15.113 -7.62) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user RX (at -15.113 -5.08) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user WKP (at -14.605 -2.54) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user DAC (at -14.605 0) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user A5 (at -15.113 2.54) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user A4 (at -15.113 5.08) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user A3 (at -15.113 7.62) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user A2 (at -15.113 10.16) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user A1 (at -15.113 12.7) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user D1 (at 13.97 12.7) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user D2 (at 13.97 10.16) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user D3 (at 13.97 7.62) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user D4 (at 13.97 5.08) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user D5 (at 13.97 2.54) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user D6 (at 13.97 0) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user D7 (at 13.97 -2.54) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user GND (at 14.478 -5.08) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user VBT (at 14.478 -7.62) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user RST (at 14.478 -10.16) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user 3V3 (at 14.478 -12.7 180) (layer B.SilkS)
    (effects (font (size 0.9652 0.9652) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user A0 (at -15.0622 15.24) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (fp_text user D0 (at 13.97 15.24 180) (layer B.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.1524)) (justify mirror))
  )
  (pad 1 thru_hole circle (at -8.89 -12.7) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at -8.89 -10.16) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at -8.89 -7.62) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3V3 thru_hole circle (at 11.43 -12.7) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at -8.89 -5.08) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at -8.89 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at -8.89 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole circle (at -8.89 2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole circle (at -8.89 5.08) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 thru_hole circle (at -8.89 7.62) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 thru_hole circle (at -8.89 10.16) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 thru_hole circle (at -8.89 12.7) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 thru_hole circle (at -8.89 15.24) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 13 thru_hole circle (at 8.89 15.24) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 14 thru_hole circle (at 8.89 12.7) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 15 thru_hole circle (at 8.89 10.16) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 16 thru_hole circle (at 8.89 7.62) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 17 thru_hole circle (at 8.89 5.08) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 18 thru_hole circle (at 8.89 2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 19 thru_hole circle (at 8.89 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 20 thru_hole circle (at 8.89 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 21 thru_hole circle (at 8.89 -5.08) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 22 thru_hole circle (at 8.89 -7.62) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 23 thru_hole circle (at 8.89 -10.16) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 24 thru_hole circle (at 8.89 -12.7) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A0 thru_hole circle (at -11.43 15.24) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A1 thru_hole circle (at -11.43 12.7) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A2 thru_hole circle (at -11.43 10.16) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A3 thru_hole circle (at -11.43 7.62) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A4 thru_hole circle (at -11.43 5.08) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A5 thru_hole circle (at -11.43 2.54) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D0 thru_hole circle (at 11.43 15.24) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D1 thru_hole circle (at 11.43 12.7) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D2 thru_hole circle (at 11.43 10.16) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D3 thru_hole circle (at 11.43 7.62) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D4 thru_hole circle (at 11.43 5.08) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D5 thru_hole circle (at 11.43 2.54) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D6 thru_hole circle (at 11.43 0) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D7 thru_hole circle (at 11.43 -2.54) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad DAC thru_hole circle (at -11.43 0) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad GND@ thru_hole circle (at -11.43 -10.16) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad GND@ thru_hole circle (at 11.43 -5.08) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad RST thru_hole circle (at 11.43 -10.16) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad RX thru_hole circle (at -11.43 -5.08) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad TX thru_hole circle (at -11.43 -7.62) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad VBAT thru_hole circle (at 11.43 -7.62) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad VIN thru_hole circle (at -11.43 -12.7) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad WKP thru_hole circle (at -11.43 -2.54) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
