(module MOLEX-1X6_LOCK (layer F.Cu) (tedit 5963E902)
  (descr "MOLEX 6-PIN PLATED THROUGH-HOLE LOCKING FOOTPRINT")
  (tags "MOLEX 6-PIN PLATED THROUGH-HOLE LOCKING FOOTPRINT")
  (attr virtual)
  (fp_text reference >NAME (at 0 -3.556) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 3.1242) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.27 -3.048) (end -1.27 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 13.97 -3.048) (end 13.97 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 13.97 -3.048) (end -1.27 -3.048) (layer F.SilkS) (width 0.127))
  (fp_line (start 13.97 2.54) (end 12.7 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 12.7 2.54) (end 0 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 2.54) (end -1.27 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 2.54) (end 0 1.27) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 1.27) (end 12.7 1.27) (layer F.SilkS) (width 0.127))
  (fp_line (start 12.7 1.27) (end 12.7 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.635 -1.27) (end 0.635 -1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 0.635 -1.27) (end -0.635 -1.27) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 2.54 0.254) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 7.62 0.254) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 10.16 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 12.7 0.254) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
