EESchema-DOCLIB  Version 2.0
#
$CMP ANTENNA-GROUNDEDTRACE-15.2MM
D Antenna w/ Ground Connection 2.4GHz antennae with signal and ground terminals. <ul><li><b>TRACE_ANTENNA_2.4GHZ_15.2MM</b> - Meander Trace antenna<ul><li>15.2 x 5.7mm footprint</li><li>Based on layout from <a href="http://www.ti.com/lit/an/swra117d/swra117d.pdf">TI app note AN043</a>.</li></ul></li><li><b>TRACE_ANTENNA_2.4GHZ_25.7MM</b> - Inverted F trace antenna<ul><li>25.7 x 7.5 mm footprint.</li><li>Based on layout from <a href="http://www.ti.com/lit/an/swru120b/swru120b.pdf">TI design note DN0007</a>.</li></ul></li></ul> 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP ANTENNA-GROUNDEDTRACE-25.7MM
D Antenna w/ Ground Connection 2.4GHz antennae with signal and ground terminals. <ul><li><b>TRACE_ANTENNA_2.4GHZ_15.2MM</b> - Meander Trace antenna<ul><li>15.2 x 5.7mm footprint</li><li>Based on layout from <a href="http://www.ti.com/lit/an/swra117d/swra117d.pdf">TI app note AN043</a>.</li></ul></li><li><b>TRACE_ANTENNA_2.4GHZ_25.7MM</b> - Inverted F trace antenna<ul><li>25.7 x 7.5 mm footprint.</li><li>Based on layout from <a href="http://www.ti.com/lit/an/swru120b/swru120b.pdf">TI design note DN0007</a>.</li></ul></li></ul> 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP ANTENNA2.4GHZ-6.5X2.2MM
D Single-ended Antennae 2.4GHz and antennae with just one terminal. These are all chip antennae. <b>2.4GHz (WiFi/BT/ZigBee) Antennae</b><ul><li><b>ANT-2.4GHZ-6.5X2.2MM</b> - 6.5 x 2.2 mm chip antenna. (<a href="https://www.sparkfun.com/products/144">SparkFun Product</a>)</li><li><b>ANT-2.4GHZ8.0X1.0MM</b> -  8.0 x 1.0 mm chip antenna. (<a href="http://www.mouser.com/ds/2/611/antenna_2500at44m0400-242425.pdf">Datasheet</a>)</li><li><b>ANT-2.4GHZ9.5X2.0MM</b> - 9.5 x 2.0 mm chip antenna. (<a href="https://www.sparkfun.com/products/9025">SparkFun Product</a>)</li></ul> 
K PROD_ID:ANT-08187
$ENDCMP
#
$CMP ANTENNA2.4GHZ-8.0X1.0MM
D Single-ended Antennae 2.4GHz and antennae with just one terminal. These are all chip antennae. <b>2.4GHz (WiFi/BT/ZigBee) Antennae</b><ul><li><b>ANT-2.4GHZ-6.5X2.2MM</b> - 6.5 x 2.2 mm chip antenna. (<a href="https://www.sparkfun.com/products/144">SparkFun Product</a>)</li><li><b>ANT-2.4GHZ8.0X1.0MM</b> -  8.0 x 1.0 mm chip antenna. (<a href="http://www.mouser.com/ds/2/611/antenna_2500at44m0400-242425.pdf">Datasheet</a>)</li><li><b>ANT-2.4GHZ9.5X2.0MM</b> - 9.5 x 2.0 mm chip antenna. (<a href="https://www.sparkfun.com/products/9025">SparkFun Product</a>)</li></ul> 
K PROD_ID:ANT-11807
$ENDCMP
#
$CMP ANTENNA2.4GHZ-9.5X2.0MM
D Single-ended Antennae 2.4GHz and antennae with just one terminal. These are all chip antennae. <b>2.4GHz (WiFi/BT/ZigBee) Antennae</b><ul><li><b>ANT-2.4GHZ-6.5X2.2MM</b> - 6.5 x 2.2 mm chip antenna. (<a href="https://www.sparkfun.com/products/144">SparkFun Product</a>)</li><li><b>ANT-2.4GHZ8.0X1.0MM</b> -  8.0 x 1.0 mm chip antenna. (<a href="http://www.mouser.com/ds/2/611/antenna_2500at44m0400-242425.pdf">Datasheet</a>)</li><li><b>ANT-2.4GHZ9.5X2.0MM</b> - 9.5 x 2.0 mm chip antenna. (<a href="https://www.sparkfun.com/products/9025">SparkFun Product</a>)</li></ul> 
K PROD_ID:ANT-09067
$ENDCMP
#
$CMP ATMEGA128RFA1
D Atmel ATmega128RFA1 8-Bit AVR Microcontroller w/ Low-Power 2.4GHz RF Transceiver The  ATmega128RFA1  is  a  low-power  CMOS  8-bit  microcontroller  based  on  the  AVR enhanced RISC architecture combined with a high data rate transceiver for the 2.4 GHz ISM band. By   executing   powerful   instructions   in   a   single   clock   cycle,   the   device   achieves  throughputs  approaching  1  MIPS  per  MHz  allowing  the  system  designer  to  optimize power consumption versus processing speed. The  radio  transceiver  provides  high  data  rates  from  250 kb/s  up  to  2 Mb/s,  frame handling,  outstanding receiver  sensitivity  and  high transmit  output  power  enabling  a very robust wireless communication.  <a href="http://www.atmel.com/Images/Atmel-8266-MCU_Wireless-ATmega128RFA1_Datasheet.pdf">Datasheet</a> <a href="https://www.sparkfun.com/products/11197">SparkFun ATmega128RFA1 Development Board</a> 
K PROD_ID:IC-09639
$ENDCMP
#
$CMP BALUN0805
D Balun Transformer to convert an unbalanced signal to a balenced one, or vice-versa. <a href="http://katalog.we-online.de/pbs/datasheet/748421245.pdf">Example Datasheet</a> 
K PROD_ID:COMP-09637
$ENDCMP
#
$CMP BC118
D Blue Creation BC118 Bluetooth 4.0 Audio Module BC118 consists of a Bluetooth Smart (Bluetooth 4.0) radio, a microprocessor running an embedded protocol stack. Themodule is controlled by high level UART instructions or GPIOs. B118 supports UART and I2C Transparent mode forcable replacement, standard/custom profiles, central and peripheral modes. It can connect to any Android, iOS orWindows Mobile Smartphone that is Bluetooth smart capable. The firmware can be upgraded using an App provided byBlueCreation. BC118 can run standalone, with a host processor or controlled by an App. <a href="http://media.digikey.com/pdf/Data%20Sheets/BlueCreation%20PDFs/BC118_DS.pdf">Datasheet</a> <b>SparkFun Products</b>:<ul><li><a href="https://www.sparkfun.com/products/13019">BLE Mate 2</a> (WRL-13019)</li></ul>
K PROD_ID:WRL-12203
$ENDCMP
#
$CMP BLUERADIO_BR-LE4.0-S2
D <H3>Blue Radios BR-LE4.0-S2A BlueTooth 4.0 Module</H3>The BR-LE4.0-S2A is a standalone Class 1 Bluetooth 4.0 module that requires no firmware or external components. Custom client applications can be written directly onto the module, which supports both analog and digital peripherals, eliminating the need for a second microprocessor. Alternately, the BR-LE4.0-S2A can be integrated into an existing design as a HCI network processor device, with a host processor running the core application and the BR-LE4.0-S2A providing Bluetooth low energy communications. <b>SparkFun Products</b>:<ul><li><a href="https://www.sparkfun.com/products/12991">Bluetooth 4.0 Module - BR-LE 4.0-S2A</a> (WRL-12991)</li></ul> 
K PROD_ID:IC-11328
$ENDCMP
#
$CMP BLUETOOTH-RN-52
D Roving Networks RN-52 Bluetooth Audio Module The RN-52 is an audio module that provides a highly integrated solution for delivering high quality stereo audio in a small form factor with little difficulty. This module is perfect for a project involving hands free audio for your car, remote controlling your media center, or streaming 2-channel audio. <b>SparkFun Products</b>:<ul><li><a href="https://www.sparkfun.com/products/11678">RN-52 - Bluetooth Audio Module</a> (WRL-11678)</li><li><a href="https://www.sparkfun.com/products/12849">Audio Bluetooth Breakout - RN-52</a> (WRL-12849)</li></ul> 
K PROD_ID:IC-11569
$ENDCMP
#
$CMP BTM-182_
D Rayson BTM-182 Bluetooth Module The BTM-182  is an easy to use Bluetooth SPP (Serial Port Protocol) module, designed for transparent wireless serial connection setup. This is a fully qualified Bluetooth V2.0+EDR (Enhanced Data Rate) 3Mbps modulation with complete 2.4GHz radio transceiver. It uses CSR Bluecore 04 external single chip Bluetooth system with CMOS technology and with AFH (Adaptive Frequency Hopping). <b>SparkFun Products</b>:<ul><li><a href="https://www.sparkfun.com/products/retired/9977">Bluetooth DIP Module - Rayson BTM-182</a> (WRL-9977)</li></ul> 
K PROD_ID:IC-09842
$ENDCMP
#
$CMP CC3000
D Texas Instruments CC3000 WiFi Module The CC3000 from TI (Texas Instruments) is a self-contained wireless network processor that makes incorporating internet connectivity into your project simple. Instead of the more standard UART communication method, the CC3000 module utilizes an SPI interface allowing you, the user, to control the flow of data as you please. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/12820">WiFi SMD Module - CC3000</a> (WRL-12820)</li><li><a href="https://www.sparkfun.com/products/12072">SparkFun WiFi Breakout - CC3000</a> (WRL-12072)</li><li><a href="https://www.sparkfun.com/products/12071">SparkFun WiFi Shield - CC3000</a> (WRL-12071)</li></ul> 
K PROD_ID:IC-12643
$ENDCMP
#
$CMP ELECTRIC_IMP
D Electric Imp SD Socket The Electric Imp provides an easy, integrated way to connect almost any hardware device both to other devices and to internet services. It s more than just a WiFi card, or even a WiFi module with processing built in - it s an integrated platform that deals with the drudgery of connectivity, allowing you to concentrate on the application instead of the mechanics.This device matches the <a href="https://www.sparkfun.com/products/11395">Electric Imp</a> pinout to a 4UCONN SD MMC connector. The 4UCONN part number for the connector is <a href="http://www.4uconnector.com/online/Itemadrawing.asp?fldseries=19646&seriesno_a=12">19646</a>. <b>SparkFun Products</b>:<ul><li><a href="https://www.sparkfun.com/products/12886">Electric Imp Breakout</a> (WRL-12886)</li><li><a href="https://www.sparkfun.com/products/12887">SparkFun Electric Imp Shield</a> (WRL-12887)</li></ul> 
K PROD_ID:CONN-11976
$ENDCMP
#
$CMP ESP32
D Espressif ESP32 <li>WiFi-compatible SoC microcontroller.</li><li> Bluetooth Low energy support (BLE, BT4.0, Bluetooth Smart)</li><li>28 GPIO pins</li><li>Dual-core Tensilica LX6 microprocessor</li><li>Hardware accelerated encryption (AES, SHA2, ECC, RSA-4096)</li><li>4MB Flash memory</li><li>520kB internal SRAM</li><li><a href= https://cdn.sparkfun.com/datasheets/IoT/esp32_datasheet_en.pdf >Datasheet</a></li> <b>SparkFun Products:</b><ul><li><a href='https://www.sparkfun.com/products/13907'>SparkFun ESP32 Thing</a></li></ul> 
K PROD_ID:IC-13338
$ENDCMP
#
$CMP ESP8266
D Espressif ESP8266 WiFi/Microcontroller SoC The ESP8266 WiFi Module is a self contained SOC with integrated TCP/IP protocol stack that can give any microcontroller access to your WiFi network. The ESP8266 is capable of either hosting an application or offloading all Wi-Fi networking functions from another application processor. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/13678">WiFi Module ESP8266</a> (WRL-13678)</li><li><a href="https://www.sparkfun.com/products/13231">SparkFun ESP8266 Thing</a> (WRL-13231)</li><li><a href="https://www.sparkfun.com/products/13287">SparkFun WiFi Shield - ESP8266</a> (WRL-13287)</li><li><a href="https://www.sparkfun.com/products/13711">SparkFun ESP8266 Thing - Dev Board</a> (WRL-13711)</li><li><a href="https://www.sparkfun.com/products/13794">SparkFun Blynk Board - ESP8266</a> (WRL-13794)</li></ul> 
K PROD_ID:IC-12452
$ENDCMP
#
$CMP ID-12_20
D ID Innovations 125kHz RFID Reader (ID2, ID3, ID12, and ID20) The IDS, ID3, ID12, and ID20 are very simple to use RFID reader modules. Power the module, hold up a 125kHz card, and get a serial string output containing the unique ID of the card. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/11862">RFID Reader ID-3LA (125 kHz)</a> (SEN-11862)</li><li><a href="https://www.sparkfun.com/products/11827">RFID Reader ID-12LA (125 kHz)</a> (SEN-11827)</li><li><a href="https://www.sparkfun.com/products/11828">RFID Reader ID-20LA (125 kHz)</a> (SEN-11828)</li><li><a href="https://www.sparkfun.com/products/9963">SparkFun RFID USB Reader</a> (SEN-9963)</li></ul> 
K PROD_ID:CONN-08875
$ENDCMP
#
$CMP ID-12_20ID-12_LOCK
D ID Innovations 125kHz RFID Reader (ID2, ID3, ID12, and ID20) The IDS, ID3, ID12, and ID20 are very simple to use RFID reader modules. Power the module, hold up a 125kHz card, and get a serial string output containing the unique ID of the card. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/11862">RFID Reader ID-3LA (125 kHz)</a> (SEN-11862)</li><li><a href="https://www.sparkfun.com/products/11827">RFID Reader ID-12LA (125 kHz)</a> (SEN-11827)</li><li><a href="https://www.sparkfun.com/products/11828">RFID Reader ID-20LA (125 kHz)</a> (SEN-11828)</li><li><a href="https://www.sparkfun.com/products/9963">SparkFun RFID USB Reader</a> (SEN-9963)</li></ul> 
K PROD_ID:CONN-08875
$ENDCMP
#
$CMP ID-12_20SMD
D ID Innovations 125kHz RFID Reader (ID2, ID3, ID12, and ID20) The IDS, ID3, ID12, and ID20 are very simple to use RFID reader modules. Power the module, hold up a 125kHz card, and get a serial string output containing the unique ID of the card. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/11862">RFID Reader ID-3LA (125 kHz)</a> (SEN-11862)</li><li><a href="https://www.sparkfun.com/products/11827">RFID Reader ID-12LA (125 kHz)</a> (SEN-11827)</li><li><a href="https://www.sparkfun.com/products/11828">RFID Reader ID-20LA (125 kHz)</a> (SEN-11828)</li><li><a href="https://www.sparkfun.com/products/9963">SparkFun RFID USB Reader</a> (SEN-9963)</li></ul> 
K PROD_ID:CONN-09345, CONN-09344
$ENDCMP
#
$CMP NRF24L01SMD
D Nordic nrf24L01 2.4GHz Low-power Transceiver This is the very popular, low cost, very low power RF transceiver from Nordic Semiconductor. Simple SPI interface. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/690">2.4GHz Transceiver IC - nRF24L01+</a> (COM-00690)</li><li><a href="https://www.sparkfun.com/products/705">SparkFun Transceiver Breakout - nRF24L01+ (RP-SMA)</a> (WRL-00705)</li><li><a href="https://www.sparkfun.com/products/691">SparkFun Transceiver Breakout - nRF24L01+</a> (COM-00691)</li></ul> 
K PROD_ID:IC-08950
$ENDCMP
#
$CMP NRF24LE1
D Nordic nRF24LE1 Ultra-low Power Wireless System on Chip The Nordic Semiconductor nRF24LE1 is a 2.4GHz ISM band radio with emhanced 8051 MCU, up to 2Mbps on air data rate, 1.9 to 3.6V supply range, 16-32-bit multiplication-division co-processor (MDU), 16 kBytes of on-chip Flash, 1 kBytes on SRAM, 1 kBytes NV data memory, 512 Bytes NV data memory (extended endurance), Interrupt controller with 18 sources and 4 priority levels, 1 Analog comparator, 10 Bit ADC, Hardware SPI slave and master, UART, three 16-bit timers/counters, AES encryption/decryption co-processor, Random number generator, 2-Wire interface, 2 Channel PWM, 7, 15, or 31 GPIO lines, On-chip hardware debug support for a JTAG debugger. 
K PROD_ID:IC-09044
$ENDCMP
#
$CMP NRF24LU1
D Nordic nRF24LU1+ Single-Chip 2.4GHz Transceiver w/ USB Microcontroller and Flash Nordic s nRF24LU1+ is a complete system-on-chip wireless transceiver. The nRF24LU1+ features a fully integrated USB 2.0 compliant device controller, which makes this chip a great choice for a compact wireless USB dongle. The nRF24LU1+ is compatible with our nRF24L01+ 2.4GHz RF transceivers as well. Additional features include an 8-bit application microcontroller, 32 kB flash memory, 6 GPIO pins, SPI and UART support, and up to 2Mbps on air data rates. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/9525">2.4GHz Transceiver IC - nRF24LU1+</a> (COM-09525)</li></ul> 
K PROD_ID:IC-09045
$ENDCMP
#
$CMP NRF52832
D Nordic nRF52832 Bluetooth Smart/ANT/2.4GHz RF SoC The nRF52832 SoC is a powerful, highly flexible ultra-low power multiprotocol SoC ideally suited for Bluetooth  Smart ANT and 2.4GHz ultra low-power wireless applications.<br>The nRF52832 SoC is built around a 32-bit ARM  Cortex -M4F CPU with 512kB + 64kB RAM. The embedded 2.4GHz transceiver supports Bluetooth Smart, ANT and proprietary 2.4 GHz protocol stack. <br>It is on air compatible with the nRF51 Series, nRF24L and nRF24AP Series products from Nordic Semiconductor. <a href="https://cdn.sparkfun.com/datasheets/Wireless/Bluetooth/nRF52832_PS_v1.0.pdf">Datasheet</a> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13990 >SparkFun nRF52832 Breakout</a></li></ul> 
K PROD_ID:IC-13460
$ENDCMP
#
$CMP RF-LINK_RX
D RF Link Receiver (434 MHz, 315 MHz) These wireless receivers work with equivalent transmitters. They can easily fit into a breadboard and work well with microcontrollers to create a very simple wireless data link. Since these are only receivers, they will only work communicating data one-way, you would need two pairs (of different frequencies) to act as a transmitter/receiver pair.. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/10532">RF Link Receiver - 4800bps (434 MHz)</a>(WRL-10532)</li></ul> 
K PROD_ID:WRL-10533
$ENDCMP
#
$CMP RF-LINK_TX
D RF Link Transmitter (434 MHz, 315 MHz) These wireless transmitters work with equivalent receivers. They can easily fit into a breadboard and work well with microcontrollers to create a very simple wireless data link. Since these are only transmitters, they will only work communicating data one-way, you would need two pairs (of different frequencies) to act as a transmitter/receiver pair. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/10534">RF Link Transmitter - 434MHz</a> (WRL-10534)</li></ul> 
K PROD_ID:WRL-10534
$ENDCMP
#
$CMP RFD77101
D <strong>Simblee   BLE Module RFD77101</strong>   2015 RF Digital Corporation<br/> <a href="https://cdn.sparkfun.com/datasheets/IoT/Simblee%20RFD77101%20Datasheet%20v1.0.pdf">Datasheet</a><br/>PATENTS PENDING 04.01.2015<br><br>Bluetooth Smart radio transceiver, ARM Cortex M0 microcontroller.<br> 128kB Flash, 24kB RAM, no EEPROM<br> Arduino-compatible.  <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13808 >Simblee BLE Module - RFD77101</a></li><li><a href= https://www.sparkfun.com/products/13632 >SparkFun Simblee BLE Breakout - RFD77101</a></li></ul> 
K PROD_ID:COMP-13237
$ENDCMP
#
$CMP RFM22434MHZ
D Hope RF RFM22 ISM Transciever Module The RFM22 is a low-power, low cost radio that is capable of operating in the 434MHz and 900MHz open bands. It's frequency is software defined and there are some very good libraries written for it. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/11018">SparkFun RFM22 Shield - 434MHz</a> (DEV-11018)</li></ul> 
K PROD_ID:IC-10007
$ENDCMP
#
$CMP RFM22915MHZ
D Hope RF RFM22 ISM Transciever Module The RFM22 is a low-power, low cost radio that is capable of operating in the 434MHz and 900MHz open bands. It's frequency is software defined and there are some very good libraries written for it. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/11018">SparkFun RFM22 Shield - 434MHz</a> (DEV-11018)</li></ul> 
K PROD_ID:IC-11750
$ENDCMP
#
$CMP RFM69CW-915MHZ
D Hope RF RFM69CW ISM Transceiver Module  The RFM69CW radio module by HopeRF is a compact, powerful radio transceiver module for swapping data packets in the 868 MHz ISM band, using standard and enhanced FSK modulation. The radio is great for sub-compact designs; just 4mm of mounted height from using an SMD precision crystal. <a href="http://www.hoperf.com/upload/rf/RFM69CW-V1.1.pdf">Datasheet</a> 
K PROD_ID:IC-11996
$ENDCMP
#
$CMP RFM69HCW-433
D Hope RF RFM69H ISM Transceiver Module  The RFM69H is a transceiver module capable of operation over a wide frequency range, including the 315,433,868 and 915MHz license-free ISM (Industry Scientific and Medical) frequency bands. All major RF communication parameters are programmable and most of them  can  be  dynamically set.  The  RFM69H  offers  the unique advantage of programmable narrow-band and wide- band  communication modes. The RFM69H is optimized for low power consumption while offering high RF output power and channelized operation.Compliance  ETSI and FCC regulations.  <a href="http://www.hoperf.cn/upload/docs/RF/SX/RFM69H_DataSheet_v1.3.pdf">Datasheet</a> <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/13909">RFM69HCW Wireless Transceiver - 915MHz</a> (COM-13909)</a></li><li><a href="https://www.sparkfun.com/products/13910">RFM69HCW Wireless Transceiver - 434MHz</a> (COM-13910)</a></li><li><a href="https://www.sparkfun.com/products/12775">SparkFun RFM69 Breakout (915MHz)</a> (WRL-12775)</a></li><li><a href="https://www.sparkfun.com/products/12823">SparkFun RFM69 Breakout (434MHz)</a> (WRL-12823)</a></li></ul> 
K PROD_ID:IC-12053
$ENDCMP
#
$CMP RFM69HCW-915
D Hope RF RFM69H ISM Transceiver Module  The RFM69H is a transceiver module capable of operation over a wide frequency range, including the 315,433,868 and 915MHz license-free ISM (Industry Scientific and Medical) frequency bands. All major RF communication parameters are programmable and most of them  can  be  dynamically set.  The  RFM69H  offers  the unique advantage of programmable narrow-band and wide- band  communication modes. The RFM69H is optimized for low power consumption while offering high RF output power and channelized operation.Compliance  ETSI and FCC regulations.  <a href="http://www.hoperf.cn/upload/docs/RF/SX/RFM69H_DataSheet_v1.3.pdf">Datasheet</a> <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/13909">RFM69HCW Wireless Transceiver - 915MHz</a> (COM-13909)</a></li><li><a href="https://www.sparkfun.com/products/13910">RFM69HCW Wireless Transceiver - 434MHz</a> (COM-13910)</a></li><li><a href="https://www.sparkfun.com/products/12775">SparkFun RFM69 Breakout (915MHz)</a> (WRL-12775)</a></li><li><a href="https://www.sparkfun.com/products/12823">SparkFun RFM69 Breakout (434MHz)</a> (WRL-12823)</a></li></ul> 
K PROD_ID:IC-11997
$ENDCMP
#
$CMP RFM69HW
D Hope RF RFM69H ISM Transceiver Module  The RFM69H is a transceiver module capable of operation over a wide frequency range, including the 315,433,868 and 915MHz license-free ISM (Industry Scientific and Medical) frequency bands. All major RF communication parameters are programmable and most of them  can  be  dynamically set.  The  RFM69H  offers  the unique advantage of programmable narrow-band and wide- band  communication modes. The RFM69H is optimized for low power consumption while offering high RF output power and channelized operation.Compliance  ETSI and FCC regulations.  <a href="http://www.hoperf.cn/upload/docs/RF/SX/RFM69H_DataSheet_v1.3.pdf">Datasheet</a> <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/13909">RFM69HCW Wireless Transceiver - 915MHz</a> (COM-13909)</a></li><li><a href="https://www.sparkfun.com/products/13910">RFM69HCW Wireless Transceiver - 434MHz</a> (COM-13910)</a></li><li><a href="https://www.sparkfun.com/products/12775">SparkFun RFM69 Breakout (915MHz)</a> (WRL-12775)</a></li><li><a href="https://www.sparkfun.com/products/12823">SparkFun RFM69 Breakout (434MHz)</a> (WRL-12823)</a></li></ul> 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP RMCM01
D Polar RMCM01 Heart Rate Monitor Receiver  The Polar heart rate receiver component receiverwirelessly receives the heart rate signal from Polartransmitter belt. The complete heart rate measurementsystem consists of three different parts; transmitter,receiver and electronics and/or display device that isoutputting the heart rate value. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/8661">Polar Heart Rate Monitor Interface</a> (SEN-08661) 
K PROD_ID:COMP-08853
$ENDCMP
#
$CMP RN171
D Roving Networks RN-171 802.11b/g WiFi Serial Module  The RN-171 is a small form factor, ultra-low power embedded TCP/IP module. The RN-171 is a standalone, complete TCP/IP wireless networking module. Due to its small form factor and extremely low power consumption, it is perfect for mobile wireless applications such as asset monitoring, sensors, and portable battery operated devices. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/retired/11049">WiFly RN-171 802.11b/g Serial Module</a> (WRL-11049)</li></ul> 
K PROD_ID:IC-11000
$ENDCMP
#
$CMP SI4703
D Silicon Labs Si4703 FM Tuner Beyond enabling you to tune in to FM radio stations, the Si4703 is also capable of detecting and processing both Radio Data Service (RDS) and Radio Broadcast Data Service (RBDS) information. The Si4703 even does a very good job of filtering and carrier detection. It also enables data such as the station ID and song name to be displayed to the user. <b>SparkFun Products</b><ul><li><a href="https://www.sparkfun.com/products/12938">SparkFun FM Tuner Evaluation Board - Si4703</a> (WRL-12938)</li><li><a href="https://www.sparkfun.com/products/11083">SparkFun FM Tuner Basic Breakout - Si4703</a> (WRL-11083)</li><li><a href="https://www.sparkfun.com/products/11043">FabFM Radio Kit </a> (KIT-11043)</li></ul> 
K PROD_ID:IC-10150
$ENDCMP
#
$CMP SM130
D SonMicro SMB130 - 13.56 MHz RFID Mifare Read/Write Module The SMB130 is a 28 pin DIP module that includes all necessary components for a 13.56 MHz RFID MIFARE , aside from a PCB antenna. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10126">RFID Module - SM130 MIFARE  (13.56 MHz) </a> (SEN-10126)</li></ul> 
K PROD_ID:LPA-12905
$ENDCMP
#
$CMP SM5100B
D LinkSprite SM5100B GSM/GPRS Module The SM5100B is a miniature, quad-band GSM 850/EGSM 900/DCS 1800/PCS 1900 module, which can be integrated into a great number of wireless projects. You can use this module to accomplish almost anything a normal cell phone can - SMS text messages, GSM/GPRS, TCP/IP, and more! <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9533">GSM/GPRS Module - SM5100B</a> (CEL-09533)</li></ul> 
K PROD_ID:CONN-09315
$ENDCMP
#
$CMP WIFLY_GSX
D Roving Networks WiFly GSX (RN-131C) Wi-Fi Module The WiFly GSX (RN-131C) module is a complete ultra low power embedded TCP/IP solution. The WiFly GSX module is a stand alone, embedded wireless 802.11b/g networking module. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10004">WiFly GSX 802.11b/g Serial Module - Roving Networks</a> (WRL-10004)</li></ul> 
K PROD_ID:IC-12671
$ENDCMP
#
$CMP XBEE
D Digi XBee and XBee Pro XBees are tiny blue chips that can communicate wirelessly with each other. They can do simple things, like replacing a couple of wires in serial communication, which is nice when you want to make a remote for your paintball vehicle. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/pages/xbee_guide">SparkFun XBee Buying Guide</a></li><li><a href="https://www.sparkfun.com/products/11812">SparkFun XBee Explorer USB</a> (WRL-11812)</li><li><a href="https://www.sparkfun.com/products/8276">Breakout Board for XBee Module</a> (WRL-8276)</li><li><a href="https://www.sparkfun.com/products/11373">SparkFun XBee Explorer Regulated</a> (WRL-11373)</li><li><a href="https://www.sparkfun.com/products/11697">SparkFun XBee Explorer Dongle</a> (WRL-11697)</li><li><a href="https://www.sparkfun.com/products/12847">SparkFun XBee Shield</a> (WRL-12847)</li><li><a href="https://www.sparkfun.com/products/13225">SparkFun XBee Explorer Serial</a> (WRL-13225)</li></ul>
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP XBEELOCK
D Digi XBee and XBee Pro XBees are tiny blue chips that can communicate wirelessly with each other. They can do simple things, like replacing a couple of wires in serial communication, which is nice when you want to make a remote for your paintball vehicle. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/pages/xbee_guide">SparkFun XBee Buying Guide</a></li><li><a href="https://www.sparkfun.com/products/11812">SparkFun XBee Explorer USB</a> (WRL-11812)</li><li><a href="https://www.sparkfun.com/products/8276">Breakout Board for XBee Module</a> (WRL-8276)</li><li><a href="https://www.sparkfun.com/products/11373">SparkFun XBee Explorer Regulated</a> (WRL-11373)</li><li><a href="https://www.sparkfun.com/products/11697">SparkFun XBee Explorer Dongle</a> (WRL-11697)</li><li><a href="https://www.sparkfun.com/products/12847">SparkFun XBee Shield</a> (WRL-12847)</li><li><a href="https://www.sparkfun.com/products/13225">SparkFun XBee Explorer Serial</a> (WRL-13225)</li></ul>
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP XBEELONGPAD
D Digi XBee and XBee Pro XBees are tiny blue chips that can communicate wirelessly with each other. They can do simple things, like replacing a couple of wires in serial communication, which is nice when you want to make a remote for your paintball vehicle. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/pages/xbee_guide">SparkFun XBee Buying Guide</a></li><li><a href="https://www.sparkfun.com/products/11812">SparkFun XBee Explorer USB</a> (WRL-11812)</li><li><a href="https://www.sparkfun.com/products/8276">Breakout Board for XBee Module</a> (WRL-8276)</li><li><a href="https://www.sparkfun.com/products/11373">SparkFun XBee Explorer Regulated</a> (WRL-11373)</li><li><a href="https://www.sparkfun.com/products/11697">SparkFun XBee Explorer Dongle</a> (WRL-11697)</li><li><a href="https://www.sparkfun.com/products/12847">SparkFun XBee Shield</a> (WRL-12847)</li><li><a href="https://www.sparkfun.com/products/13225">SparkFun XBee Explorer Serial</a> (WRL-13225)</li></ul>
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP XBEESILK
D Digi XBee and XBee Pro XBees are tiny blue chips that can communicate wirelessly with each other. They can do simple things, like replacing a couple of wires in serial communication, which is nice when you want to make a remote for your paintball vehicle. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/pages/xbee_guide">SparkFun XBee Buying Guide</a></li><li><a href="https://www.sparkfun.com/products/11812">SparkFun XBee Explorer USB</a> (WRL-11812)</li><li><a href="https://www.sparkfun.com/products/8276">Breakout Board for XBee Module</a> (WRL-8276)</li><li><a href="https://www.sparkfun.com/products/11373">SparkFun XBee Explorer Regulated</a> (WRL-11373)</li><li><a href="https://www.sparkfun.com/products/11697">SparkFun XBee Explorer Dongle</a> (WRL-11697)</li><li><a href="https://www.sparkfun.com/products/12847">SparkFun XBee Shield</a> (WRL-12847)</li><li><a href="https://www.sparkfun.com/products/13225">SparkFun XBee Explorer Serial</a> (WRL-13225)</li></ul>
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP XBEESMD
D Digi XBee and XBee Pro XBees are tiny blue chips that can communicate wirelessly with each other. They can do simple things, like replacing a couple of wires in serial communication, which is nice when you want to make a remote for your paintball vehicle. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/pages/xbee_guide">SparkFun XBee Buying Guide</a></li><li><a href="https://www.sparkfun.com/products/11812">SparkFun XBee Explorer USB</a> (WRL-11812)</li><li><a href="https://www.sparkfun.com/products/8276">Breakout Board for XBee Module</a> (WRL-8276)</li><li><a href="https://www.sparkfun.com/products/11373">SparkFun XBee Explorer Regulated</a> (WRL-11373)</li><li><a href="https://www.sparkfun.com/products/11697">SparkFun XBee Explorer Dongle</a> (WRL-11697)</li><li><a href="https://www.sparkfun.com/products/12847">SparkFun XBee Shield</a> (WRL-12847)</li><li><a href="https://www.sparkfun.com/products/13225">SparkFun XBee Explorer Serial</a> (WRL-13225)</li></ul>
K PROD_ID:CONN-09042
$ENDCMP
#
$CMP XTEND-DIGI-MODEM
D Digi XTend 900 1W RF Transceiver The XTend Modem packs a ton of RF punch into a small, low-power, easy-to-use, and reliable module. Outdoors, with line-of-sight, this module can communicate at up to 40 miles; indoors it can still do up to 3000ft. The module transfers a standard asynchronous serial data stream, operates within the ISM 900MHz frequency band and sustains up to 115.2kbps data throughput. The module comes with an attached RPSMA antenna connector. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9411">XTend 900 1W RPSMA - 40 Mile Range</a> (WRL-09411)</li></ul>
K PROD_ID:WRL-09411
$ENDCMP
#
#End Doc Library
