(module CPOL-RADIAL-5MM-10MM (layer F.Cu) (tedit 200000)
  (descr "5 MM SPACED PTHS IN 10 MM DIAMETER SILK RING")
  (tags "5 MM SPACED PTHS IN 10 MM DIAMETER SILK RING")
  (attr virtual)
  (fp_text reference >NAME (at 0 -5.588) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 5.588) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.905 -2.54) (end -3.175 -2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.175 -2.54) (end 1.905 -2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.54 -3.175) (end 2.54 -1.905) (layer F.SilkS) (width 0.2032))
  (fp_circle (center 0 0) (end 0 -4.99872) (layer F.SilkS) (width 0.2032))
  (pad + thru_hole rect (at 2.49936 0) (size 1.9304 1.9304) (drill 0.89916) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad - thru_hole circle (at -2.49936 0) (size 1.9304 1.9304) (drill 0.89916) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
