EESchema-DOCLIB  Version 2.0
#
$CMP 555D
D General purpose bipolar Timer <a href="http://www.sparkfun.com/datasheets/Components/General/ne555.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12707">SparkFun SparkPunk Sequencer Kit</a> (KIT-12707)</li><li><a href="https://www.sparkfun.com/products/9273">Storefront Component: 555 Timer</a> (COM-09273)</li></ul>Two parts valid for production:<br><br>VFP: IC-11930 (M7555 PTH)<br>VFP: IC-09173 (555 PTH) - <b>Preferred</b><br>
K PROD_ID:NA-XXXXX
$ENDCMP
#
$CMP 555KIT
D General purpose bipolar Timer <a href="http://www.sparkfun.com/datasheets/Components/General/ne555.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12707">SparkFun SparkPunk Sequencer Kit</a> (KIT-12707)</li><li><a href="https://www.sparkfun.com/products/9273">Storefront Component: 555 Timer</a> (COM-09273)</li></ul>Two parts valid for production:<br><br>VFP: IC-11930 (M7555 PTH)<br>VFP: IC-09173 (555 PTH) - <b>Preferred</b><br>
K PROD_ID:IC-09173
$ENDCMP
#
$CMP 555P
D General purpose bipolar Timer <a href="http://www.sparkfun.com/datasheets/Components/General/ne555.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12707">SparkFun SparkPunk Sequencer Kit</a> (KIT-12707)</li><li><a href="https://www.sparkfun.com/products/9273">Storefront Component: 555 Timer</a> (COM-09273)</li></ul>Two parts valid for production:<br><br>VFP: IC-11930 (M7555 PTH)<br>VFP: IC-09173 (555 PTH) - <b>Preferred</b><br>
K PROD_ID:IC-09173
$ENDCMP
#
$CMP 556
D 556 Dual 555 timer 2 555 timers in one package<br>1MHZ 14DIP <a href="https://cdn.sparkfun.com/datasheets/Kits/icm7555-56.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11177">SparkFun SparkPunk Sound Kit</a> (KIT-11177)</li></ul>
K PROD_ID:IC-11898
$ENDCMP
#
$CMP 556KIT
D 556 Dual 555 timer 2 555 timers in one package<br>1MHZ 14DIP <a href="https://cdn.sparkfun.com/datasheets/Kits/icm7555-56.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11177">SparkFun SparkPunk Sound Kit</a> (KIT-11177)</li></ul>
K PROD_ID:IC-11898
$ENDCMP
#
$CMP A4988
D DMOS Microstepping Driver with Translator(IC-11483)
K PROD_ID:IC-11483
$ENDCMP
#
$CMP AD5262
D Digital Potentiometer IC <a href="https://cdn.sparkfun.com/assets/learn_tutorials/1/8/8/AD5262BRU_datasheet.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13144">SparkFun Touch Potentiometer</a> (PRT-13144)</li></ul>
K PROD_ID:IC-12358
$ENDCMP
#
$CMP AD9837
D Programmable waveform generator Sine, triangular, and square wave outputs <a href="https://cdn.sparkfun.com/datasheets/BreakoutBoards/AD9837.PDF">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11420">SparkFun MiniGen - Pro Mini Signal Generator Shield</a> (BOB-11420)</li></ul>
K PROD_ID:IC-11223
$ENDCMP
#
$CMP AL8805
D Constant current LED driver PWM-able 1MHz switch freq 6V-36V<br>Up to 1A LED current
K PROD_ID:IC-11626
$ENDCMP
#
$CMP ATAES132
D Crypto 32Kb Serial EEPROM AES-128-CCM<br>MAC<br>Secure Storage for 128-bit keys<br>Encrypted User Memory Readn and Write<br>HWRNG<br>2.5V to 5.5V<br> <a href="https://cdn.sparkfun.com/datasheets/Dev/Beagle/Atmel-8760-CryptoAuth-ATAES132-Datasheet.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12773">CryptoCape</a> (DEV-12773)</li><li><a href="https://www.sparkfun.com/products/13183">SparkFun CryptoShield</a> (DEV-13183)</li></ul>
K PROD_ID:IC-11983
$ENDCMP
#
$CMP ATECC108
D ATECC108 ECDSA with NIST ATECC108: Provides ECDSA with NIST curves P256, B283, and K283.  Also, a RNG, 8.5Kb EEPROM.  2.0V - 5.5V. <a href="https://cdn.sparkfun.com/datasheets/Dev/Beagle/Atmel-8873S-CryptoAuth-ATECC108-Datasheet-Summary.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12773">CryptoCape</a> (DEV-12773)</li><li><a href="https://www.sparkfun.com/products/13183">SparkFun CryptoShield</a> (DEV-13183)</li></ul>
K PROD_ID:IC-11982
$ENDCMP
#
$CMP ATSHA204-TSU
D Atmel ATSHA204 The Atmel ATSHA204 is an optimized authentication chip that includes a 4.5Kb EEPROM. This array can be used for storage of keys, miscellaneous read/write, read-only, password or secret data, and consumption tracking. Access to the various sections of memory can be restricted in a variety of ways and then the configuration locked to prevent changes. <a href="http://www.atmel.com/Images/Atmel-8740-CryptoAuth-ATSHA204-Datasheet.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12887">SparkFun Electric Imp Shield</a> </li><li><a href="https://www.sparkfun.com/products/12886"> SparkFun Electric Imp Breakout</a></li></ul>
K PROD_ID:IC-11208
$ENDCMP
#
$CMP ATSHA204_SOIC8
D Crypto 4.5KB I2C <a href="https://cdn.sparkfun.com/datasheets/Dev/Beagle/Atmel-8740-CryptoAuth-ATSHA204-Datasheet.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12773">CryptoCape</a> (DEV-12773)</li><li><a href="https://www.sparkfun.com/products/13183">SparkFun CryptoShield</a> (DEV-13183)</li></ul>
K PROD_ID:IC-11981
$ENDCMP
#
$CMP DRV883X
D DRV8835 2 Channel Motor Driver Dual 1.5A H-bridge, 2-11V<li><a href= http://www.ti.com/lit/ds/symlink/drv8835.pdf >Datasheet</a></li> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13911 >SparkFun Serial Controlled Motor Driver</a></li></ul> 
K PROD_ID:IC-13342
$ENDCMP
#
$CMP INA169
D Current Output Current Shunt Monitor 0.5%, SOT23-5 <a href="http://cdn.sparkfun.com/datasheets/Sensors/Current/ina169.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12040">SparkFun Current Sensor Breakout - INA169</a> (SEN-12040)</li></ul>
K PROD_ID:IC-11776
$ENDCMP
#
$CMP L298
D L298 Dual Full Bridge Driver
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP L298HEATSINK
D L298 Dual Full Bridge Driver
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP L298_BRIDGE_DRIVER
D Full-bridge power driver IC
K PROD_ID:IC-09133
$ENDCMP
#
$CMP L298_SMD_W_PAD
D Full-bridge power driver ICThis device uses the ground pad under the IC
K PROD_ID:IC-09133
$ENDCMP
#
$CMP L6470
D 3A RMS/7A peak bipolar stepper motor driver with SPI control<br>and step input in HTSSOP-28 package.<br>IC-10648
K PROD_ID:IC-10648
$ENDCMP
#
$CMP LM391N
D LM3914 Dot/Bar Display Driver TTL/CMOS Logic<br>Drives LEDs, LCDs, Vacuum Fluorecents<br>Source:<br><a href="http://www.national.com/ds/LM/LM3915.pdf"> Data sheet LM3915</a><br><a href="http://www.national.com/ds/LM/LM3914.pdf"> Data sheet LM3914 </a> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13688 >MyoWare LED Shield</a></li><li><a href= https://www.sparkfun.com/products/12694 >Dot/Bar Display Driver - LM3914</a></li></ul> 
K PROD_ID:COM-12694
$ENDCMP
#
$CMP LM391V
D LM3914 Dot/Bar Display Driver TTL/CMOS Logic<br>Drives LEDs, LCDs, Vacuum Fluorecents<br>Source:<br><a href="http://www.national.com/ds/LM/LM3915.pdf"> Data sheet LM3915</a><br><a href="http://www.national.com/ds/LM/LM3914.pdf"> Data sheet LM3914 </a> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13688 >MyoWare LED Shield</a></li><li><a href= https://www.sparkfun.com/products/12694 >Dot/Bar Display Driver - LM3914</a></li></ul> 
K PROD_ID:
$ENDCMP
#
$CMP LP55231WQFN
D LP55231 Programmable 9-Output LED Driver <li><a href= http://www.ti.com/lit/ds/symlink/lp55231.pdf >Datasheet</a></li> <b>SparkFun Products:</b><ul><li><a href='https://www.sparkfun.com/products/13884'>SparkFun LED Driver Breakout - LP55231</a></li></ul> 
K PROD_ID:IC-13302
$ENDCMP
#
$CMP MCP41XXX
D Digital Potentiometer - 10K SPI controlled single digital potentiometer by Microchip <a href="http://cdn.sparkfun.com/datasheets/Components/General%20IC/22060b.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10613">Storefront component: Digital Potentiometer - 10K</a> (COM-10613)</li></ul>
K PROD_ID:NA-XXXXX
$ENDCMP
#
$CMP MCP41XXXDIL
D Digital Potentiometer - 10K SPI controlled single digital potentiometer by Microchip <a href="http://cdn.sparkfun.com/datasheets/Components/General%20IC/22060b.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10613">Storefront component: Digital Potentiometer - 10K</a> (COM-10613)</li></ul>
K PROD_ID:RES-13155
$ENDCMP
#
$CMP MSGEQ7DIL
D 7-band graphic equalizer This IC is for making a 7 band/channel audio spectrometer.<br>There are two versions of this part.  The DIP available on the storefront, and the SO used in product.<a href="https://www.sparkfun.com/datasheets/Components/General/MSGEQ7.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10468">Storefront component: Graphic Equalizer Display Filter - MSGEQ7</a> (COM-10468)</li><li><a href="https://www.sparkfun.com/products/13116">SparkFun Spectrum Shield</a> (DEV-13116)</li></ul>
K PROD_ID:IC-12196
$ENDCMP
#
$CMP MSGEQ7SOIC
D 7-band graphic equalizer This IC is for making a 7 band/channel audio spectrometer.<br>There are two versions of this part.  The DIP available on the storefront, and the SO used in product.<a href="https://www.sparkfun.com/datasheets/Components/General/MSGEQ7.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10468">Storefront component: Graphic Equalizer Display Filter - MSGEQ7</a> (COM-10468)</li><li><a href="https://www.sparkfun.com/products/13116">SparkFun Spectrum Shield</a> (DEV-13116)</li></ul>
K PROD_ID:IC-10141
$ENDCMP
#
$CMP PCA9685
D 16-channel 12-bit PWM I<sup>2</sup>C interface<br>Internal Oscillator 40Hz to 1kHz<br>Can be totem pole or open collector<br>2.3V to 5.5V <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13042">SparkFun Block for Intel  Edison - PWM</a> (DEV-13042)</li></ul>PROTO: IC-12240<br>PROD_ID: IC-12271
K PROD_ID:IC-12271
$ENDCMP
#
$CMP SPEAKJETDIP
D Speech synthesis chip <a href="http://www.sparkfun.com/datasheets/Components/General/speakjet-usermanual.pdf">User Manual</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9578">SpeakJet</a> (COM-09578)</li></ul>
K PROD_ID:IC-09512
$ENDCMP
#
$CMP SPEAKJETSMD
D Speech synthesis chip <a href="http://www.sparkfun.com/datasheets/Components/General/speakjet-usermanual.pdf">User Manual</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9578">SpeakJet</a> (COM-09578)</li></ul>
K PROD_ID:IC-XXXXX
$ENDCMP
#
$CMP STA540
D Multiwatt package for L298 bridge driver
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP STA5406400BG_W_SOLDERPOSTS
D Multiwatt package for L298 bridge driver
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP STA540W_6400BG_HEATSINK
D Multiwatt package for L298 bridge driver
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP STA540W_YB324G_HEATSINK
D Multiwatt package for L298 bridge driver
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP SX1509
D Semtech SX1509 The SX1509 is a complete ultra low voltage 1.2V to 3.6V General Purpose parallel Input/Output (GPIO) expanders ideal for low power handheld battery powered equipment. This version comes in a 16-channel configuration and allows easy serial expansion of I/O through a standard 400kHz I2C interface. GPIO devices can provide additional control and monitoring when the microcontroller or chipset has insufficient I/O ports, or in systems where serial communication and control from a remote location is advantageous. <a href="http://cdn.sparkfun.com/datasheets/BreakoutBoards/sx1509.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13601">SparkFun 16 Output I/O Expander Breakout - SX1509</a> (BOB-13601)</li><li><a href="https://www.sparkfun.com/products/13582">SparkFun Line Follower Array</a> (SEN-13582)</li></ul>
K PROD_ID:IC-11311
$ENDCMP
#
$CMP TB6612FNG
D Toshiba 1A dual motor driverIC-09363
K PROD_ID:IC-09363
$ENDCMP
#
$CMP TS3USB221A
D DPDT Analog Mux DPDT Analog Mux<br>Vcc 2.5 to 3.3V<br>Passes up to 5.5V at 3.3V supply<br>900MHz BW, 6&#8486; switch resistance<br> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12935">SparkFun FTDI SmartBasic</a> (DEV-12935)</li></ul>
K PROD_ID:IC-12115
$ENDCMP
#
$CMP ULN2803DIP
D <b>Darlington Driver(IC-07959, low stock)</b>ULN2803 Darlington array. 500mA max per channel, 8-channel package. Spark Fun Electronics SKU : COM-00312
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP ULN2803SOIC
D <b>Darlington Driver(IC-07959, low stock)</b>ULN2803 Darlington array. 500mA max per channel, 8-channel package. Spark Fun Electronics SKU : COM-00312
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP ULN2803SOICW
D <b>Darlington Driver(IC-07959, low stock)</b>ULN2803 Darlington array. 500mA max per channel, 8-channel package. Spark Fun Electronics SKU : COM-00312
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP VNH2SP30
D 30A motor driver IC(IC-10030,moster moto)
K PROD_ID:XXX-00000
$ENDCMP
#
#End Doc Library
