(module CPOL-RADIAL-2.5MM-6.5MM (layer F.Cu) (tedit 200000)
  (descr "2.5 MM SPACED PTHS WITH 6.5 MM DIAMETER OUTLINE")
  (tags "2.5 MM SPACED PTHS WITH 6.5 MM DIAMETER OUTLINE")
  (attr virtual)
  (fp_text reference >NAME (at 0 -3.81) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 3.81) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -0.635 -1.778) (end -1.905 -1.778) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.905 -1.778) (end 0.635 -1.778) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.27 -2.413) (end 1.27 -1.143) (layer F.SilkS) (width 0.2032))
  (fp_circle (center 0 0) (end 0 -3.24866) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole rect (at 1.24968 0) (size 1.651 1.651) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at -1.24968 0) (size 1.651 1.651) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
