(module ESP32_THING (layer F.Cu) (tedit 200000)
  (descr "SPARKFUN ESP32 THING BOARD")
  (tags "SPARKFUN ESP32 THING BOARD")
  (attr virtual)
  (fp_text reference >NAME (at 12.7 -2.54) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 12.7 -1.27) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 0 0) (end 0 -51.435) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 0 -51.435) (end 0 -58.293) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 0.635 -58.928) (end 24.765 -58.928) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 25.4 -58.293) (end 25.4 -51.435) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 25.4 -51.435) (end 25.4 0) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 25.4 0) (end 0 0) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 0 -51.435) (end 25.4 -51.435) (layer Dwgs.User) (width 0.127))
  (fp_line (start 0 -51.435) (end 25.4 -51.435) (layer F.SilkS) (width 0.127))
  (fp_line (start 25.4 -51.435) (end 25.4 -58.928) (layer F.SilkS) (width 0.127))
  (fp_line (start 25.4 -58.928) (end 0 -58.928) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 -58.928) (end 0 -51.435) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 -51.435) (end 25.4 -51.435) (layer F.SilkS) (width 0.127))
  (fp_line (start 25.4 -51.435) (end 25.4 -58.928) (layer F.SilkS) (width 0.127))
  (fp_line (start 25.4 -58.928) (end 0 -58.928) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 -58.928) (end 0 -51.435) (layer F.SilkS) (width 0.127))
  (fp_arc (start 0.635 -58.293) (end 0 -58.293) (angle 90) (layer Dwgs.User) (width 0.2032))
  (fp_arc (start 24.765 -58.293) (end 24.765 -58.928) (angle 90) (layer Dwgs.User) (width 0.2032))
  (fp_text user 34 (at 3.81 -34.4805) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 35 (at 3.81 -31.9405) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 32 (at 3.81 -39.55796) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 33 (at 3.81 -37.0205) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 25 (at 3.81 -29.4005) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 26 (at 3.81 -26.85796) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 27 (at 3.7846 -24.3205) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 14 (at 3.7846 -21.7805) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 12 (at 3.7846 -19.2405) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 13 (at 3.81 -16.8275) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user VBAT (at 4.699 -6.6675) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 19 (at 20.9169 -36.7665) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 21 (at 20.9169 -46.9265) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 22 (at 20.9423 -39.30396) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user RX (at 20.9677 -41.8465) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user TX (at 20.9169 -44.3865) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 23 (at 20.9169 -34.2265) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 18 (at 20.9169 -31.6865) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 5 (at 20.4724 -29.1465) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 15 (at 20.9169 -26.60396) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 2 (at 20.4724 -24.0665) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 0 (at 20.4724 -21.5265) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 4 (at 20.4724 -18.9865) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 17 (at 20.9169 -16.4465) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 16 (at 20.9169 -13.9065) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 39 (at 3.81 -42.1005) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 38 (at 3.81 -44.6405) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 37 (at 3.81 -47.1805) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 36 (at 3.81 -49.7205) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user GND (at 21.2852 -49.4665) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user !RST! (at 5.1435 -14.2875) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 3V3 (at 4.2545 -11.7475) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user GND (at 4.2545 -9.2075) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user VUSB (at 4.699 -4.12496) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user GND (at 4.2545 -1.5875) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user 3V3 (at 21.3614 -11.3665) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user GND (at 21.3614 -8.8265) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user VBAT (at 21.8059 -6.2865) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user VUSB (at 21.8059 -3.7465) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user GND (at 21.3614 -1.2065) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.127)))
  )
  (fp_text user "Antenna Keepout" (at 12.7 -55.245) (layer Dwgs.User)
    (effects (font (size 0.889 0.889) (thickness 0.0762)))
  )
  (pad 1 thru_hole rect (at 1.27 -1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 1.27 -3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 1.27 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 1.27 -8.89) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 1.27 -11.43) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 1.27 -13.97) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole circle (at 1.27 -16.51) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole circle (at 1.27 -19.05) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 thru_hole circle (at 1.27 -21.59) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 thru_hole circle (at 1.27 -24.13) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 thru_hole circle (at 1.27 -26.67) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 thru_hole circle (at 1.27 -29.21) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 13 thru_hole circle (at 1.27 -31.75) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 14 thru_hole circle (at 1.27 -34.29) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 15 thru_hole circle (at 1.27 -36.83) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 16 thru_hole circle (at 1.27 -39.37) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 17 thru_hole circle (at 1.27 -41.91) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 18 thru_hole circle (at 1.27 -44.45) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 19 thru_hole circle (at 1.27 -46.99) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 20 thru_hole circle (at 1.27 -49.53) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 21 thru_hole circle (at 24.13 -49.53) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 22 thru_hole circle (at 24.13 -46.99) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 23 thru_hole circle (at 24.13 -44.45) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 24 thru_hole circle (at 24.13 -41.91) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 25 thru_hole circle (at 24.13 -39.37) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 26 thru_hole circle (at 24.13 -36.83) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 27 thru_hole circle (at 24.13 -34.29) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 28 thru_hole circle (at 24.13 -31.75) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 29 thru_hole circle (at 24.13 -29.21) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 30 thru_hole circle (at 24.13 -26.67) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 31 thru_hole circle (at 24.13 -24.13) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 32 thru_hole circle (at 24.13 -21.59) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 33 thru_hole circle (at 24.13 -19.05) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 34 thru_hole circle (at 24.13 -16.51) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 35 thru_hole circle (at 24.13 -13.97) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 36 thru_hole circle (at 24.13 -11.43) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 37 thru_hole circle (at 24.13 -8.89) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 38 thru_hole circle (at 24.13 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 39 thru_hole circle (at 24.13 -3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 40 thru_hole rect (at 24.13 -1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
