EESchema-DOCLIB  Version 2.0
#
$CMP ADP160
D Nanopower LDO<br>Iq less than 1uA for low Iload
K PROD_ID:VREG-11306
$ENDCMP
#
$CMP AP2202-ADJ
D AP2202 Adjustable LDO<br>Diodes Inc small, low-cost LDO<br>150mA, 13.2V, less than 200mV dropout
K PROD_ID:VREG-12189
$ENDCMP
#
$CMP BQ24075
D Texas Instruments BQ24075 LiPo Battery Chargerand Power-Path Management IC The bq2407x series of devices are integrated Li-Ion linear chargers and system power path management devices targeted at space-limited portable applications. The devices operate from either a USB port or an AC adapter and support charge currents up to 1.5 A. The input voltage range with input overvoltage protection supports unregulated adapters. The USB input current limit accuracy and start up sequence allow the bq2407x to meet USB-IF inrush current specifications. Additionally, the input dynamic power management (VIN-DPM) prevents the charger from crashing incorrectly configured USB sources. <a href="http://www.ti.com/product/BQ24075/datasheet">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13777">SparkFun Battery Babysitter</a> (PRT-13777)</li></ul>
K PROD_ID:IC-13219
$ENDCMP
#
$CMP BQ27441-G1
D Texas Instruments BQ27441-G1 LiPo Battery Fuel Gauge The Texas Instruments bq27441-G1 fuel gauge is a microcontroller peripheral that provides system-side fuel gauging for single-cell Li-Ion batteries. The device requires minimal user configuration and system microcontroller firmware development. The bq27441-G1 battery fuel gauge uses the patented Impedance Track  algorithm for fuel gauging, and provides information such as remaining battery capacity (mAh), state-of-charge (%), and battery voltage (mV). <a href="http://www.ti.com/product/BQ27441-G1/datasheet">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13777">SparkFun Battery Babysitter</a> (PRT-13777)</li></ul>
K PROD_ID:IC-13220
$ENDCMP
#
$CMP DC-DC_CONVERTER
D APTS006A0X-SRZ (IC-09258) Step-down 6A variable voltage switching module (TOL-09275)
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP LM25011
D The LM25011 constant on-time step-down switching regulatorfeatures all the functions needed to implement a low-cost, efficient, buck bias regulator capable of supplying up to 2 A of load current. This high-voltage regulator contains an N-Channel Buck switch, a startup regulator, current limit detection, and internal ripple control.
K PROD_ID:IC-12528
$ENDCMP
#
$CMP LM3880_-QI
D LM3880 Simple Power Sequencer <ul><li>Precision enable pin & 3 open-drain output flags</li><li>Input Voltage Range of 2.7 V to 5.5 V</li><li>Power-Up and Power-Down Control</li><li>The timing sequence of the LM3880 is controlled entirely by the enable (EN) pin. Upon power up, all the flags are held low until this precision enable is pulled high</li></ul> LM3880MF-1XY (Timing Designator)<ul><li>AF: 16ms</li><li>AE: 2ms</li><li>AA: 10ms</li><li>AB: 30ms</li><li>AC: 60ms</li><li>AD: 120ms</li></ul> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13303">SparkFun 6 Degrees of Freedom Breakout - LSM303C</a> (BOB-13303)</li></ul>
K PROD_ID:IC-12558
$ENDCMP
#
$CMP LT3652
D <H3>LT3652 MPPT Solar Charge Controller(IC-11822) 5V-32V smart charger for batteries up to 14.4V
K PROD_ID:LT3652
$ENDCMP
#
$CMP LTC3588_
D Energy Harvesting Power Supply(IC-09818)
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP LTC4150
D LTC4150 Coulomb Counter / Battery Gas Gauge <ul><li>Indicates Charge Quantity and Polarity</li><li> 50mV Sense Voltage Range</li><li>Precision Timer Capacitor or Crystal Not Required</li><li>2.7V to 8.5V Operation</li><li>High Side Sense</li><li>32.55Hz/V Charge Count Frequency</li><li>1.5 A Shutdown Current</li><li>10-Pin MSOP Package</li></ul>  <a href="https://cdn.sparkfun.com/datasheets/BreakoutBoards/LTC4150fc.pdf">Datasheet</a><br>Manufacturer's page: <a href="http://www.linear.com/product/LTC4150">http://www.linear.com/product/LTC4150</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12052">SparkFun Coulomb Counter Breakout - LTC4150</a> (BOB-12052)</li></ul>
K PROD_ID:IC-11785
$ENDCMP
#
$CMP MAX17048DFN8
D Micropower 1-Cell Li+ ModelGauge <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13614">Qduino Mini</a> (DEV-13614)</li></ul>
K PROD_ID:IC-12551
$ENDCMP
#
$CMP MAX1704X
D MAX17043/MAX17044: Battery Fuel Guage (43 is 1cell, 44 is 2cell)
K PROD_ID:IC-10399
$ENDCMP
#
$CMP MC34063DIP
D Jellybean switching supply controller (IC-11612, also SF)
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP MC34063SMD
D Jellybean switching supply controller (IC-11612, also SF)
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP MCP73831
D MCP73831T Li-Ion, Li-Pol Controller Miniature single cell, fully integrated Li-Ion, Li-polymer charge management controller<li><a href= http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf >Datasheet</a></li> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13907 >SparkFun ESP32 Thing</a></li><li><a href= https://www.sparkfun.com/products/14001 >SparkFun 9DoF Razor IMU M0</a></li></ul> 
K PROD_ID:IC-09995
$ENDCMP
#
$CMP MCP7384XX
D Li-Ion charge controller family from Microchip (IC-08344)
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP PAM2401
D PAM2401 - Boost PMIC Specifications:<ul><li>Up to 1A output current</li><li>0.9V to 4.75V Input Range </li><li>2.5V to 5.0V Adjustable Output Voltage</li></ul> <a href= https://www.diodes.com/assets/Datasheets/PAM2401.pdf >Datasheet</a> (Diodes inc.) </ul> 
K PROD_ID:IC-XXXXX
$ENDCMP
#
$CMP R-78E5.0-1.0
D <H3>Recom Power 5V 1A DC/DC Converter</H3>The Recom R-78E5.0-X.X is a compact DC/DC converter module that is a pin for pin drop-in replacement for the LM7805 linear voltage regulator. <br><br>Specifications:<ul><li>Input Range: 7-28V</li><li>Output Voltage: 5V</li><li>Output Current: 1A</li><li>Max Efficiency: 91%</li></ul><b><br><a href="https://www.recom-power.com/pdf/Innoline/R-78Exx-1.0.pdf">Datasheet</a>
K PROD_ID:COM-13655
$ENDCMP
#
$CMP SPX29302
D 3A LDO regulator
K PROD_ID:VREG-08337
$ENDCMP
#
$CMP TPS61200
D DC to DC Booster<br>IC-10035
K PROD_ID:IC-10035
$ENDCMP
#
$CMP TPS62065
D TPS62065 DC/DC step-Down regulator.
K PROD_ID:IC-12273
$ENDCMP
#
$CMP TPS62133RGTT
D 3-17V, 2A Step Down Converter(IC-11155)
K PROD_ID:IC-11155
$ENDCMP
#
$CMP TPS62172
D Texas Instruments TPS62172 3-17V 0.5A Step-Down Converter with DCS control. Available in adjustable and fixed output voltage versions.<br><br>Is packaged in an 8-pin WSON package measuring 2   2 mm (DSG).<br> <br>See a 3.3V fixed output version of this chip in action on the <a href="https://www.sparkfun.com/products/11400">Electric Imp Breakout Board</a>.<br><br><a href="http://www.ti.com/lit/gpn/tps62172">Datasheet</a>
K PROD_ID:IC-11307
$ENDCMP
#
$CMP V_REG_317DPACK
D <b>Voltage Regulator</b>Standard LM317 adjustable voltage regulator. AOI (Adjust Output Input). Google 'LM317 Calculator' for easy to use app to get the two resistor values needed. 240/720 for 5V output. 240/390 for 3.3V output. Spark Fun Electronics SKU : COM-00527
K PROD_ID:IC-09888
$ENDCMP
#
$CMP V_REG_317SINK
D <b>Voltage Regulator</b>Standard LM317 adjustable voltage regulator. AOI (Adjust Output Input). Google 'LM317 Calculator' for easy to use app to get the two resistor values needed. 240/720 for 5V output. 240/390 for 3.3V output. Spark Fun Electronics SKU : COM-00527
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP V_REG_317SMD
D <b>Voltage Regulator</b>Standard LM317 adjustable voltage regulator. AOI (Adjust Output Input). Google 'LM317 Calculator' for easy to use app to get the two resistor values needed. 240/720 for 5V output. 240/390 for 3.3V output. Spark Fun Electronics SKU : COM-00527
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP V_REG_78XX-TO-220
D <b>Voltage Regulator</b>Standard 78xx regulator. IGO (Input Ground Output). Spark Fun Electronics SKU : COM-00107
K PROD_ID:VREG-08450
$ENDCMP
#
$CMP V_REG_78XX7812
D <b>Voltage Regulator</b>Standard 78xx regulator. IGO (Input Ground Output). Spark Fun Electronics SKU : COM-00107
K PROD_ID:VREG-12370
$ENDCMP
#
$CMP V_REG_78XXSIDE
D <b>Voltage Regulator</b>Standard 78xx regulator. IGO (Input Ground Output). Spark Fun Electronics SKU : COM-00107
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP V_REG_78XXSINK
D <b>Voltage Regulator</b>Standard 78xx regulator. IGO (Input Ground Output). Spark Fun Electronics SKU : COM-00107
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP V_REG_78XXTO-92_UNTESTED
D <b>Voltage Regulator</b>Standard 78xx regulator. IGO (Input Ground Output). Spark Fun Electronics SKU : COM-00107
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP V_REG_AP2112K-3.3V
D AP2112 - 600mA CMOS LDO Regulator w/ Enable The AP2112 is CMOS process low dropout linear regulator with enable function, the regulator delivers a guaranteed 600mA (min.) continuous load current. Features<br><ul><li>Output Voltage Accuracy:  1.5% </li><li>Output Current: 600mA (Min.) </li><li>Foldback Short Current Protection: 50mA </li><li>Enable Function to Turn ON/OFF VOUT</li><li>Low Dropout Voltage (3.3V): 250mV (Typ.) @IOUT=600mA </li><li>Excellent Load Regulation: 0.2%/A (Typ.) </li><li>Excellent Line Regulation: 0.02%/V (Typ.) </li><li>Low Quiescent Current: 55 A (Typ.)</li><li>Low Standby Current: 0.01 A (Typ.)</li><li>Low Output Noise: 50 VRMS </li><li>PSRR: 100Hz -65dB, 1kHz -65dB </li><li> OTSD Protection </li><li>Stable  with  1.0 F Flexible Cap: Ceramic, Tantalum and Aluminum Electrolytic </li><li>Operation Temperature Range: -40 C to 85 C </li><li>ESD: MM 400V, HBM 4000V</li></ul> 
K PROD_ID:VREG-12457
$ENDCMP
#
$CMP V_REG_LD1085D2
D LD1085 3A low-drop positive voltage regulator, adjustable(VREG-10397) The LD1085xx is a low drop voltage regulator able to provide up to 3 A of output current. Dropout is guaranteed at a maximum of 1.2 V at the maximum output current, decreasing at lower loads. The LD1085xx is pin to pin compatible with the older 3-terminal adjustable regulators, but has better performances in term of drop and output tolerance.<br><br><B>Available Packages</b><ul><li>D<sup>2</sup>PAK/A - 3-pin w/ tabs, SMD
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP V_REG_LD1117VXX
D LD1117VXX voltage regulator. We carry the 3.3V version (COM-00526) in TO-220 package.
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP V_REG_LM1117SOT223
D <b>Voltage Regulator LM1117</b>Standard adjustable voltage regulator but in SMD form. Spark Fun Electronics SKU : COM-00595
K PROD_ID:VREG-08170
$ENDCMP
#
$CMP V_REG_MIC52053.3V
D <b>V_REG MIC5205</b> Standard 3.3V, 5V, and Adjustable 150mA LDO voltage regulator in SOT-23 layout. Micrel part MIC5205. BP (by-pass) pin is used to lower output noise with 470pF cap, may be left open. On the adjustable version BP is used to set output.
K PROD_ID:VREG-00822
$ENDCMP
#
$CMP V_REG_MIC52055V
D <b>V_REG MIC5205</b> Standard 3.3V, 5V, and Adjustable 150mA LDO voltage regulator in SOT-23 layout. Micrel part MIC5205. BP (by-pass) pin is used to lower output noise with 470pF cap, may be left open. On the adjustable version BP is used to set output.
K PROD_ID:VREG-00823
$ENDCMP
#
$CMP V_REG_MIC5205ADJ
D <b>V_REG MIC5205</b> Standard 3.3V, 5V, and Adjustable 150mA LDO voltage regulator in SOT-23 layout. Micrel part MIC5205. BP (by-pass) pin is used to lower output noise with 470pF cap, may be left open. On the adjustable version BP is used to set output.
K PROD_ID:VREG-12594
$ENDCMP
#
$CMP V_REG_MIC5216
D 500mA LDO, MSOP8 for better dissipation
K PROD_ID:IC-09527
$ENDCMP
#
$CMP V_REG_MIC52193.3V
D <b>V_REG MIC5219</b>Standard 3.3V and 5V 500mA LDO voltage regulator in SOT-23 layout. Micrel part MIC5219. BP (by-pass) pin is used to lower output noise with 470pF cap, may be left open.
K PROD_ID:VREG-09872
$ENDCMP
#
$CMP V_REG_MIC52195V
D <b>V_REG MIC5219</b>Standard 3.3V and 5V 500mA LDO voltage regulator in SOT-23 layout. Micrel part MIC5219. BP (by-pass) pin is used to lower output noise with 470pF cap, may be left open.
K PROD_ID:VREG-10107
$ENDCMP
#
$CMP V_REG_NCP50X
D NCP550x 500mA LDO Voltage Regulator(IC-10378)
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP V_REG_SP6214-1.8V
D Voltage Regulator - SP6214 SP6214 Series SC-70-5 Micropower SC-70 100 mA CMOS LDO Regulator<br><a href= https://www.exar.com/content/document.ashx?id=654 >Datasheet</a> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13720 >MP3 Trigger</a></li><li><a href= https://www.sparkfun.com/products/14045 >SparkFun Particle Sensor Breakout</a></li></ul> 
K PROD_ID:VREG-08428
$ENDCMP
#
$CMP V_REG_SPX3819-SOT23-5
D SPX3819 Voltage Regulator  3.3V 500mA, 16V input <a href= https://www.exar.com/content/document.ashx?id=22106 >Datasheet</a> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13911 >SparkFun Serial Controlled Motor Driver</a></li></ul> 
K PROD_ID:VREG-13321
$ENDCMP
#
#End Doc Library
