EESchema-DOCLIB  Version 2.0
#
$CMP CD4013
D Dual D-type Flip-Flop <a href="https://cdn.sparkfun.com/datasheets/Kits/CD4013B.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11177">SparkFun SparkPunk Sound Kit</a> (KIT-11177)</li><li><a href="https://www.sparkfun.com/products/12707">SparkFun SparkPunk Sequencer Kit</a> (KIT-12707)</li></ul>
K PROD_ID:IC-11896
$ENDCMP
#
$CMP CD4017
D 10-Out Decade Counter <a href="https://cdn.sparkfun.com/datasheets/Kits/cd4022b.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12707">SparkFun SparkPunk Sequencer Kit</a> (KIT-12707)</li></ul>
K PROD_ID:IC-11929
$ENDCMP
#
$CMP CD4017KIT
D 10-Out Decade Counter <a href="https://cdn.sparkfun.com/datasheets/Kits/cd4022b.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12707">SparkFun SparkPunk Sequencer Kit</a> (KIT-12707)</li></ul>
K PROD_ID:IC-11929
$ENDCMP
#
$CMP TPIC6C596SOIC
D Serial in shift register with open collector outputs This can sink up to 100mA per channel <a href="https://cdn.sparkfun.com/datasheets/Widgets/TPIC6C596.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13279">SparkFun Large Digit Driver</a> (WIG-13279)</li></ul>
K PROD_ID:IC-12522
$ENDCMP
#
#End Doc Library
