(module SWITCH_TOGGLE_SPST_RIGHT_ANGLE (layer F.Cu) (tedit 5A4D281F)
  (fp_text reference REF** (at 0 -1.27) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SWITCH_TOGGLE_SPST_RIGHT_ANGLE (at 0 -2.54) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "Front Edge" (at 0 12.7) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.81 13.88) (end -3.81 13.88) (layer Dwgs.User) (width 0.15))
  (pad 1 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -2.54 5.08) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 2.54 5.08) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
)
