(module RJ11-6 (layer F.Cu) (tedit 200000)
  (descr "RJ11 6-PIN SOCKET WITH PCB MOUNTING POST")
  (tags "RJ11 6-PIN SOCKET WITH PCB MOUNTING POST")
  (attr virtual)
  (fp_text reference >NAME (at -7.493 -8.89 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 7.493 -8.89 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 6.858 5.207) (end 6.858 -10.414) (layer F.SilkS) (width 0.2032))
  (fp_line (start 6.858 -10.414) (end -6.858 -10.414) (layer F.SilkS) (width 0.2032))
  (fp_line (start -6.858 -10.414) (end -6.858 5.207) (layer F.SilkS) (width 0.2032))
  (fp_line (start 6.858 5.207) (end -6.858 5.207) (layer F.SilkS) (width 0.2032))
  (fp_line (start -6.858 5.207) (end -6.858 8.128) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -6.858 8.128) (end 6.858 8.128) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 6.858 8.128) (end 6.858 5.207) (layer Dwgs.User) (width 0.2032))
  (pad 1 thru_hole circle (at -3.175 -8.89) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at -1.905 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at -0.635 -8.89) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 0.635 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 1.905 -8.89) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 3.175 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at -5.08 0) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 5.08 0) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
